{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[1,2,1,4],[4,1,4,2],[5,1,18,1],[3,1,3,2]]}
[]
[null,null,"UART Baud Rate Divisors"]
[]
[null,"Serial Clock",null,7372800,1843200]
[null,"Baud Clock",null,{"$f":"D4/16","v":460800},{"$f":"E4/16","v":115200}]
[null,"Baud Rate",110,{"$f":"D$5/$C6","v":4189.090909090909},{"$f":"E$5/$C6","v":1047.2727272727273}]
[null,null,300,{"$f":"D$5/$C7","v":1536},384]
[null,null,600,768,192]
[null,null,1200,384,96]
[null,null,2400,192,48]
[null,null,4800,96,24]
[null,null,9600,48,12]
[null,null,14400,32,8]
[null,null,19200,24,6]
[null,null,38400,12,3]
[null,null,57600,8,2]
[null,null,115200,4,1]
[null,null,230400,2,0.5]
[null,null,460800,1,0.25]