{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[[26,1,26,2],[27,1,40,1],[6,6,19,6],[27,6,40,6],[1,2,1,5],[4,1,4,2],[24,1,24,2],[24,3,24,5],[25,1,25,2],[6,1,19,1],[3,3,3,5],[3,1,3,2],[5,1,5,2]]}
[]
[null,null,"Possible SIO + CTC Baud Rates"]
[]
[null,null,null,"SIO Divisor"]
[null,"Serial Clock",null,64,32,16]
[null,7372800,null,{"$f":"$B6/D5","v":115200},{"$f":"$B6/E5","v":230400},460800]
[null,"Baud Rate",110,{"$f":"D$6/$C7","v":1047.2727272727273},{"$f":"E$6/$C7","v":2094.5454545454545},4189.090909090909,"CTC Divisor"]
[null,null,300,{"$f":"D$6/$C8","v":384},768,1536]
[null,null,600,192,384,768]
[null,null,1200,96,192,384]
[null,null,2400,48,96,192]
[null,null,4800,24,48,96]
[null,null,9600,12,24,48]
[null,null,14400,8,16,32]
[null,null,19200,6,12,24]
[null,null,38400,3,6,12]
[null,null,57600,2,4,8]
[null,null,115200,1,2,4]
[null,null,230400,0.5,1,2]
[null,null,460800,0.25,0.5,1]
[]
[]
[]
[]
[null,null,null,"SIO Divisor"]
[null,"Serial Clock",null,64,32,16]
[null,1843200,null,{"$f":"$B27/D26","v":28800},57600,115200]
[null,"Baud Rate",110,{"$f":"D$27/$C28","v":261.81818181818181},{"$f":"E$27/$C28","v":523.63636363636363},1047.2727272727273,"CTC Divisor"]
[null,null,300,{"$f":"D$27/$C29","v":96},192,384]
[null,null,600,48,96,192]
[null,null,1200,24,48,96]
[null,null,2400,12,24,48]
[null,null,4800,6,12,24]
[null,null,9600,3,6,12]
[null,null,14400,2,4,8]
[null,null,19200,1.5,3,6]
[null,null,38400,0.75,1.5,3]
[null,null,57600,0.5,1,2]
[null,null,115200,0.25,0.5,1]
[null,null,230400,0.125,0.25,0.5]
[null,null,460800,6.25E-2,0.125,0.25]