{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":58,"n_cols":12,"rows_kept":58,"cut":false,"hidden":false,"merged":[[5,11,22,11],[5,0,22,0],[3,2,3,10],[3,0,3,1],[4,0,4,1],[28,5,28,6],[28,3,28,4],[28,1,28,2],[28,7,28,9],[1,1,1,10],[26,1,26,10]]}
[]
[null,"Z180 Serial (ASCI) Baud Rates by Clock Rate"]
[]
[null,null,"CPU Clock PHI (MHz)"]
[null,null,6.1439999999999992,7.3727999999999998,9.2159999999999993,12.287999999999998,14.7456,18.431999999999999,24.575999999999997,{"$f":"G5*2","v":29.491199999999999},36.863999999999997]
["Z180 ASCI Divisors",122880,{"$f":"(C$5*1000000)/$B6","v":49.999999999999993},60,75,99.999999999999986,120,150,199.99999999999997,240,300,"Serial Port Baud Rate"]
[null,61440,99.999999999999986,120,150,199.99999999999997,240,300,399.99999999999994,480,600]
[null,40960,149.99999999999997,180,225,299.99999999999994,360,450,599.99999999999989,720,900]
[null,30720,199.99999999999997,240,300,399.99999999999994,480,600,799.99999999999989,960,1200]
[null,20480,299.99999999999994,360,450,599.99999999999989,720,900,1199.9999999999998,1440,1800]
[null,15360,399.99999999999994,480,600,799.99999999999989,960,1200,1599.9999999999998,1920,2400]
[null,10240,599.99999999999989,720,900,1199.9999999999998,1440,1800,2399.9999999999995,2880,3600]
[null,7680,799.99999999999989,960,1200,1599.9999999999998,1920,2400,3199.9999999999995,3840,4800]
[null,5120,1199.9999999999998,1440,1800,2399.9999999999995,2880,3600,4799.9999999999991,5760,7200]
[null,3840,1599.9999999999998,1920,2400,3199.9999999999995,3840,4800,6399.9999999999991,7680,9600]
[null,2560,{"$f":"(C$5*1000000)/$B16","v":2399.9999999999995},2880,3600,4799.9999999999991,5760,7200,9599.9999999999982,11520,14400]
[null,1920,3199.9999999999995,3840,4800,6399.9999999999991,7680,9600,12799.999999999998,15360,19200]
[null,1280,4799.9999999999991,5760,7200,9599.9999999999982,11520,14400,19199.999999999996,23040,28800]
[null,960,6399.9999999999991,7680,9600,12799.999999999998,15360,19200,25599.999999999996,30720,38400]
[null,640,9599.9999999999982,11520,14400,19199.999999999996,23040,28800,38399.999999999993,46080,57600]
[null,480,12799.999999999998,15360,19200,25599.999999999996,30720,38400,51199.999999999993,61440,76800]
[null,320,19199.999999999996,23040,28800,38399.999999999993,46080,57600,76799.999999999985,92160,115200]
[null,160,38399.999999999993,46080,57600,76799.999999999985,92160,115200,153599.99999999997,184320,230400]
[]
[null,"ASCI Baud = CPU Clock (PHI) / ASCI Divisor"]
[]
[null,"Z180 Serial (ASCI) Programming (CNTLB Values)"]
[]
[null,"Prescale (PS)",null,"Divide Ratio (DR)",null,"Speed Select (SS)",null,"CNTLB (--P-DSSS)",null,null,"Final"]
[null,"Value","Divisor","Value","Divisor","Value","Divisor","Decimal","Hex","Binary","Divisor"]
[null,0,10,0,16,0,1,{"$f":"(B31*32)+(D31*8)+F31","v":0},{"$f":"DEC2HEX(H31,2)","v":"00"},{"$f":"DEC2BIN(H31,8)","v":"00000000"},{"$f":"C31*E31*G31","v":160}]
[null,0,10,0,16,1,2,{"$f":"(B32*32)+(D32*8)+F32","v":1},{"$f":"DEC2HEX(H32,2)","v":"01"},{"$f":"DEC2BIN(H32,8)","v":"00000001"},{"$f":"C32*E32*G32","v":320}]
[null,0,10,0,16,2,4,{"$f":"(B33*32)+(D33*8)+F33","v":2},"02","00000010",{"$f":"C33*E33*G33","v":640}]
[null,0,10,0,16,3,8,{"$f":"(B34*32)+(D34*8)+F34","v":3},"03","00000011",{"$f":"C34*E34*G34","v":1280}]
[null,0,10,0,16,4,16,{"$f":"(B35*32)+(D35*8)+F35","v":4},"04","00000100",{"$f":"C35*E35*G35","v":2560}]
[null,0,10,0,16,5,32,{"$f":"(B36*32)+(D36*8)+F36","v":5},"05","00000101",{"$f":"C36*E36*G36","v":5120}]
[null,0,10,0,16,6,64,{"$f":"(B37*32)+(D37*8)+F37","v":6},"06","00000110",{"$f":"C37*E37*G37","v":10240}]
[null,0,10,1,64,0,1,{"$f":"(B38*32)+(D38*8)+F38","v":8},"08","00001000",{"$f":"C38*E38*G38","v":640}]
[null,0,10,1,64,1,2,{"$f":"(B39*32)+(D39*8)+F39","v":9},"09","00001001",{"$f":"C39*E39*G39","v":1280}]
[null,0,10,1,64,2,4,{"$f":"(B40*32)+(D40*8)+F40","v":10},"0A","00001010",{"$f":"C40*E40*G40","v":2560}]
[null,0,10,1,64,3,8,{"$f":"(B41*32)+(D41*8)+F41","v":11},"0B","00001011",{"$f":"C41*E41*G41","v":5120}]
[null,0,10,1,64,4,16,{"$f":"(B42*32)+(D42*8)+F42","v":12},"0C","00001100",{"$f":"C42*E42*G42","v":10240}]
[null,0,10,1,64,5,32,{"$f":"(B43*32)+(D43*8)+F43","v":13},"0D","00001101",{"$f":"C43*E43*G43","v":20480}]
[null,0,10,1,64,6,64,{"$f":"(B44*32)+(D44*8)+F44","v":14},"0E","00001110",{"$f":"C44*E44*G44","v":40960}]
[null,1,30,0,16,0,1,{"$f":"(B45*32)+(D45*8)+F45","v":32},"20","00100000",{"$f":"C45*E45*G45","v":480}]
[null,1,30,0,16,1,2,{"$f":"(B46*32)+(D46*8)+F46","v":33},"21","00100001",{"$f":"C46*E46*G46","v":960}]
[null,1,30,0,16,2,4,{"$f":"(B47*32)+(D47*8)+F47","v":34},"22","00100010",{"$f":"C47*E47*G47","v":1920}]
[null,1,30,0,16,3,8,{"$f":"(B48*32)+(D48*8)+F48","v":35},"23","00100011",{"$f":"C48*E48*G48","v":3840}]
[null,1,30,0,16,4,16,{"$f":"(B49*32)+(D49*8)+F49","v":36},"24","00100100",{"$f":"C49*E49*G49","v":7680}]
[null,1,30,0,16,5,32,{"$f":"(B50*32)+(D50*8)+F50","v":37},"25","00100101",{"$f":"C50*E50*G50","v":15360}]
[null,1,30,0,16,6,64,{"$f":"(B51*32)+(D51*8)+F51","v":38},"26","00100110",{"$f":"C51*E51*G51","v":30720}]
[null,1,30,1,64,0,1,{"$f":"(B52*32)+(D52*8)+F52","v":40},"28","00101000",{"$f":"C52*E52*G52","v":1920}]
[null,1,30,1,64,1,2,{"$f":"(B53*32)+(D53*8)+F53","v":41},"29","00101001",{"$f":"C53*E53*G53","v":3840}]
[null,1,30,1,64,2,4,{"$f":"(B54*32)+(D54*8)+F54","v":42},"2A","00101010",{"$f":"C54*E54*G54","v":7680}]
[null,1,30,1,64,3,8,{"$f":"(B55*32)+(D55*8)+F55","v":43},"2B","00101011",{"$f":"C55*E55*G55","v":15360}]
[null,1,30,1,64,4,16,{"$f":"(B56*32)+(D56*8)+F56","v":44},"2C","00101100",{"$f":"C56*E56*G56","v":30720}]
[null,1,30,1,64,5,32,{"$f":"(B57*32)+(D57*8)+F57","v":45},"2D","00101101",{"$f":"C57*E57*G57","v":61440}]
[null,1,30,1,64,6,64,{"$f":"(B58*32)+(D58*8)+F58","v":46},"2E","00101110",{"$f":"C58*E58*G58","v":122880}]